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the hashemite kingdom of jordan
the jordanian electric power company limited

Specification JEP 74/2026

tender document for

PG Clamps For AAA and acsr conductors



	Tenderer's Name:
	____________________

	Address:

	____________________
____________________

	Closing Date:
	____________________

	Closing Time:
	____________________


october   2026
THE JORDANIAN ELECTRIC POWER COMPANY LIMITED

AMMAN   –  JORDAN

	Telephone 962 6 5503600
P.O. BOX 618

ZIP CODE 11118
	____________
	CABLE: ELECTRICO

FAX 962 6 5503618


SPECIFICaTION  JEp 74/2026
PG Clamps For AAA and acsr conductors
1. GENERAL

The required PG clamps shall be manufactured to the latest International or equivalent national standards.
The body of PG clamps and the pressure pad plate shall be manufactured from high strength and very corrosion resisting aluminum alloy and shall withstand short circuit of 16KA for 1 second, and shall be complete with the following specifications:
· The body and pressure pad plate shall be made of high strength aluminum alloy.
· Bolts, nuts and spring washers shall be hot dip galvanized steel and of grade 8.8 and shall comply with DIN 933.
· Hexagonal nuts shall be tightly pressed into lower clamp body. Such that when the bolt is fastened, the nut remains fixed (immovable).
2. SCOPE OF WORK

The works shall comprise the design, manufacture, works testing, supply and delivery to Aqaba port, The Hashemite Kingdom of Jordan of following PG clamps.
	ITEM NO.
	Equipment
	Qty

	1.
	2 - BOLTS, AL-P.G. CLAMPS SIZE:  AL (16-70) mm2/AL (16-70) mm2. BOLT SIZE: M8
Min. dimensions 40X40mm2
Tightening torque of the screw shall not less than 35N.M. 
	50,000


NOTES:

· Documents to be submitted as an integral part of the offer, and to be evaluated with the tender:

1. Full technical details, drawings and catalogues.

2. Fully detailed reference list with contact details.
3. Complete Test certificates from reputable well recognized third party labratory to ensure that the clamps comply with the requirements of this specification.
4. ISO certificate and any documents that will assist in the evaluation.
· 2 - Non-returnable representative samples for each item above shall be submitted with the offer. Failure to submit the samples or failure of the samples will entitle JEPCO to reject the offer.
· The above item shall be provided with a bar code of 128 type C that represents the primary and secondary number of these items, as shown in the table below:
	Item No.
	Item Code

	1.
	20004002


SCHEDULE (A) 
MANUFACTURERS AND PLACES OF MANUFACTURE,
TESTING AND INSPECTION

	Item

No.
	
Description
	Manufacturer
	Place of

Manufacture
	Place of Testing & Inspection

	1.
	2 - BOLTS, AL-P.G. CLAMPS SIZE:  AL (16-70) mm2/AL (16-70) mm2. BOLT SIZE: M8
Min. dimensions 40X40mm2
Tightening torque of the screw shall not less than 35N.M. 
	……………..
	……………..
	……………..


SCHEDULE (B) 
TECHNICAL DATA
	No.
	DESCRIBTION
	UNIT
	Item 1

	1.
	CLAMP BODY.
	
	

	
	a) Material of body.

b) Grade of Al.
	
	-------------------

	
	c) No. of bolts per clamp body.
	
	-------------------

	
	d) The maximum tightening torque that the body of the clamp can withstand without breaking or deteriotating the bolts.
	N.m
	-------------------

	
	e) short circuit current / duration.
f) Dimensions.
	KA/Sec
mmXmm
	-------------------

	2.
	CLAMP BOLTS AND NUTS
	
	

	
	a) Material of bolts and nuts (specify the grade).
	
	-------------------

	
	b) Size of bolt.
	
	-------------------

	
	c) Size of the specified bolt.
	
	-------------------

	
	d) Are nuts pressed into lower clamp body? 
	Yes/No
	-------------------

	
	e) Are the bolts and nuts hot-dip galvanized?
	Yes/No
	-------------------

	3.
	PRESSURE PAD AND SPRING WASHERS.
	
	

	
	a) Is each clamp equipped with pressure pad and spring washers?
	Yes/No
	-------------------

	
	b) Material of pressure pads.
	
	-------------------

	
	c) Material of spring washers.
	
	-------------------

	4.
	CONDUCTOR MATERIAL.
	
	

	
	Main:
	
	-------------------

	
	Tap:
	
	-------------------

	5.
	CONDUCTOR CROSS SECTION.
	
	

	
	Main:
	
	-------------------

	
	Tap:
	
	-------------------


Summary Schedule

Technical and Commercial Data

Note: The following schedule represents the most essential data based on which the evaluation process shall be performed.
	item
	Description
	Quantity
	Unit CFR to Aqaba Port Price/ Currency
	Total CFR to Aqaba Port Price/ Currency
	Delivery

(Weeks)

	1.
	2 - BOLTS, AL-P.G. CLAMPS SIZE:  AL (16-70) mm2/AL (16-70) mm2. BOLT SIZE: M8 
	50,000
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